<?xml version="1.0" encoding="utf-8"?>
<C>
  <CatSec Id="M-0083_CS-SG01" Name="System Devices" Number="SG01" VisibleDescription="" DefaultLanguage="en-US" NonRegRelevantDataVersion="3">
    <CatSec Id="M-0083_CS-SG01-IP02" Name="IP Interfaces" Number="IP02" DefaultLanguage="en-US">
      <CITEM Id="M-0083_H-135-3_HP-0137-20-7EB2_CI-SCN.2DIP000.2E03-1" Name="SCN-IP000.03 Email for IP Interface with Secure" Number="1" VisibleDescription="Email function and time server" ProductRefId="M-0083_H-135-3_P-SCN.2DIP000.2E03" Hardware2ProgramRefId="M-0083_H-135-3_HP-0137-20-7EB2" DefaultLanguage="en-US" />
      <CITEM Id="M-0083_H-135-3-O0072_HP-0138-21-F18E-O0072_CI-SCN.2DIP000.2E03-1" Name="SCN-IP000.03 IP Interface with Secure" Number="1" VisibleDescription="IP Interface with IP Secure and Data Secure" ProductRefId="M-0083_H-135-3-O0072_P-SCN.2DIP000.2E03" Hardware2ProgramRefId="M-0083_H-135-3-O0072_HP-0138-21-F18E-O0072" DefaultLanguage="en-US" />
    </CatSec>
  </CatSec>
  <CatSec Id="M-0083_CS-A.2001" Name="Actuators" Number="A 01" DefaultLanguage="en-US" NonRegRelevantDataVersion="2">
    <CatSec Id="M-0083_CS-A.2001-S.2002" Name="Switch Actuators, compact version" Number="S 02" DefaultLanguage="en-US">
      <CITEM Id="M-0083_H-3.2E10-2_HP-000A-21-6D9A_CI-AKK.2D1616.2E03-1" Name="AKK-1616.03 Switch Actuator 16fold, 8SU, 16A" Number="1" VisibleDescription="Compact version, 230VAC, 16A, 70µF" ProductRefId="M-0083_H-3.2E10-2_P-AKK.2D1616.2E03" Hardware2ProgramRefId="M-0083_H-3.2E10-2_HP-000A-21-6D9A" DefaultLanguage="en-US" />
    </CatSec>
    <CatSec Id="M-0083_CS-A.2001-LA.2001" Name="LED Actuators" Number="LA 01" DefaultLanguage="en-US">
      <CITEM Id="M-0083_H-3.2E65-1_HP-0040-24-52B5_CI-AKD.2D0424R2.2E02-1" Name="AKD-0424R2.02 LED Controler 4 Ch/RGBW, 2DU MDRC" Number="1" VisibleDescription="Control RGBW LED stripes, MDRC" ProductRefId="M-0083_H-3.2E65-1_P-AKD.2D0424R2.2E02" Hardware2ProgramRefId="M-0083_H-3.2E65-1_HP-0040-24-52B5" DefaultLanguage="en-US" />
      <CITEM Id="M-0083_H-3.2E65-1_HP-0040-25-F9E1_CI-AKD.2D0424R2.2E02-1" Name="AKD-0424R2.02 LED Controler 4 Ch/RGBW, 2DU MDRC" Number="1" VisibleDescription="Control RGBW LED stripes, MDRC" ProductRefId="M-0083_H-3.2E65-1_P-AKD.2D0424R2.2E02" Hardware2ProgramRefId="M-0083_H-3.2E65-1_HP-0040-25-F9E1" DefaultLanguage="en-US" />
    </CatSec>
    <CatSec Id="M-0083_CS-A.2001-J.20ST.2001" Name="Shutter Actuator" Number="J ST 01" VisibleDescription="" DefaultLanguage="en-US">
      <CITEM Id="M-0083_H-42-49_HP-002A-38-E69D_CI-JAL.2D0210.2E02-1" Name="JAL-0210.02 Shutter Actuator 2-fold, 2SU, 230VAC" Number="1" VisibleDescription="for 230VAC shutter motors up to 600W" ProductRefId="M-0083_H-42-49_P-JAL.2D0210.2E02" Hardware2ProgramRefId="M-0083_H-42-49_HP-002A-38-E69D" DefaultLanguage="en-US" />
    </CatSec>
  </CatSec>
  <CatSec Id="M-0083_CS-B.2001" Name="Binary Input" Number="B 01" VisibleDescription="Binary input" DefaultLanguage="en-US">
    <CatSec Id="M-0083_CS-B.2001-B.20UE.2001" Name="Universal Input" Number="B UE 01" VisibleDescription="" DefaultLanguage="en-US">
      <CITEM Id="M-0083_H-178-0_HP-00B2-30-A16E_CI-BE.2D08230.2E02-1" Name="BE-08230.02 Binary Input 8-fold, 4SU, Inputs 230VAC" Number="1" VisibleDescription="Input detection of 230VAC signals" ProductRefId="M-0083_H-178-0_P-BE.2D08230.2E02" Hardware2ProgramRefId="M-0083_H-178-0_HP-00B2-30-A16E" DefaultLanguage="en-US" />
      <CITEM Id="M-0083_H-178-0_HP-00B2-32-B4D6_CI-BE.2D08230.2E02-1" Name="BE-08230.02 Binary Input 8-fold, 4SU, Inputs 230VAC" Number="1" VisibleDescription="Input detection of 230VAC signals" ProductRefId="M-0083_H-178-0_P-BE.2D08230.2E02" Hardware2ProgramRefId="M-0083_H-178-0_HP-00B2-32-B4D6" DefaultLanguage="en-US" />
    </CatSec>
  </CatSec>
  <CatSec Id="M-0083_CS-B.20TA.2001" Name="MDT Push Button" Number="B TA 01" DefaultLanguage="en-US">
    <CatSec Id="M-0083_CS-B.20TA.2001-B.20TA.2006" Name="MDT Push button 6-fold" Number="B TA 06" VisibleDescription="" DefaultLanguage="en-US">
      <CITEM Id="M-0083_H-371-0_HP-0021-15-72DF_CI-BE.2DTA5506.2E01-1" Name="BE-TA5506.01 Push button 6-fold" Number="1" VisibleDescription="Push button 6-fold standard" ProductRefId="M-0083_H-371-0_P-BE.2DTA5506.2E01" Hardware2ProgramRefId="M-0083_H-371-0_HP-0021-15-72DF" DefaultLanguage="en-US" />
    </CatSec>
    <CatSec Id="M-0083_CS-B.20TA.2001-B.20TA.2008" Name="MDT Push button 8-fold" Number="B TA 08" VisibleDescription="" DefaultLanguage="en-US">
      <CITEM Id="M-0083_H-36-1_HP-0024-15-EF03_CI-BE.2DTA55P8.2E01-1" Name="BE-TA55P8.01 Push button 8-fold / Plus" Number="1" VisibleDescription="Push button 8-fold with LED, Logic" ProductRefId="M-0083_H-36-1_P-BE.2DTA55P8.2E01" Hardware2ProgramRefId="M-0083_H-36-1_HP-0024-15-EF03" DefaultLanguage="en-US" />
    </CatSec>
    <CatSec Id="M-0083_CS-B.20TA.2001-B.20SM.2012" Name="Push Button Smart 86" Number="B SM 12" DefaultLanguage="en-US">
      <CITEM Id="M-0083_H-2.2E37-1_HP-008A-25-6CE4_CI-BE.2DTAS86T.2E01-1" Name="BE-TAS86T.01 Push Button Smart 86 with temperature sensor" Number="1" VisibleDescription="12fold, Slap function, Temperature measurement" ProductRefId="M-0083_H-2.2E37-1_P-BE.2DTAS86T.2E01" Hardware2ProgramRefId="M-0083_H-2.2E37-1_HP-008A-25-6CE4" DefaultLanguage="en-US" />
    </CatSec>
  </CatSec>
  <CatSec Id="M-0083_CS-ST01" Name="Control" Number="ST01" DefaultLanguage="en-US">
    <CatSec Id="M-0083_CS-ST01-ZSU01" Name="Time Switch" Number="ZSU01" DefaultLanguage="en-US">
      <CITEM Id="M-0083_H-74-0_HP-0055-14-CE77_CI-SCN.2DRTC20.2E01-1" Name="Time Switch 20-channel with LCD display" Number="1" VisibleDescription="Weekly time switching with 10 channels" ProductRefId="M-0083_H-74-0_P-SCN.2DRTC20.2E01" Hardware2ProgramRefId="M-0083_H-74-0_HP-0055-14-CE77" DefaultLanguage="en-US" />
      <CITEM Id="M-0083_H-274-1_HP-0255-20-5A67_CI-SCN.2DRTC20.2E02-1" Name="SCN-RTC20.02 Time Switch 20-channel with colour display" Number="1" ProductRefId="M-0083_H-274-1_P-SCN.2DRTC20.2E02" Hardware2ProgramRefId="M-0083_H-274-1_HP-0255-20-5A67" DefaultLanguage="en-US" />
    </CatSec>
    <CatSec Id="M-0083_CS-ST01-STL01" Name="Logic Module" Number="STL01" DefaultLanguage="en-US">
      <CITEM Id="M-0083_H-2.2E80-1_HP-004B-20-7B3F_CI-SCN.2DLOG1.2E02-2" Name="SCN-LOG1.02 Logic Module" Number="2" ProductRefId="M-0083_H-2.2E80-1_P-SCN.2DLOG1.2E02" Hardware2ProgramRefId="M-0083_H-2.2E80-1_HP-004B-20-7B3F" DefaultLanguage="en-US" />
    </CatSec>
  </CatSec>
  <CatSec Id="M-0083_CS-BP01" Name="Motion / Presence Detector" Number="BP01" DefaultLanguage="en-US">
    <CatSec Id="M-0083_CS-BP01-P02" Name="Presence Detector" Number="P02" DefaultLanguage="en-US">
      <CITEM Id="M-0083_H-323-3_HP-0075-42-B02B_CI-SCN.2DP360K3.2E03-1" Name="SCN-P360K3.03 Presence Detector 360° CL 3S" Number="1" VisibleDescription="Presence Detector 360°, Ceiling mounting, CL 3 Sensors" ProductRefId="M-0083_H-323-3_P-SCN.2DP360K3.2E03" Hardware2ProgramRefId="M-0083_H-323-3_HP-0075-42-B02B" DefaultLanguage="en-US" />
      <CITEM Id="M-0083_H-323-3_HP-0075-44-2007_CI-SCN.2DP360K3.2E03-1" Name="SCN-P360K3.03 Presence Detector 360° CL 3S" Number="1" VisibleDescription="Presence Detector 360°, Ceiling mounting, CL 3 Sensors" ProductRefId="M-0083_H-323-3_P-SCN.2DP360K3.2E03" Hardware2ProgramRefId="M-0083_H-323-3_HP-0075-44-2007" DefaultLanguage="en-US" />
    </CatSec>
  </CatSec>
  <CatSec Id="M-0083_CS-AR01" Name="Archive" Number="AR01" DefaultLanguage="en-US" NonRegRelevantDataVersion="1">
    <CatSec Id="M-0083_CS-AR01-WS" Name="Weather Sensors" Number="WS" DefaultLanguage="en-US">
      <CatSec Id="M-0083_CS-AR01-WS-SS" Name="Sun Sensor" Number="SS" DefaultLanguage="en-US">
        <CITEM Id="M-0083_H-78-1_HP-004E-10-8D83_CI-SCN.2DSS1H.2E01-2" Name="SCN-SS1H.01 Sun sensor" Number="2" VisibleDescription="Sun sensor, Facade control" ProductRefId="M-0083_H-78-1_P-SCN.2DSS1H.2E01" Hardware2ProgramRefId="M-0083_H-78-1_HP-004E-10-8D83" DefaultLanguage="en-US" />
      </CatSec>
    </CatSec>
  </CatSec>
</C>