<?xml version="1.0" encoding="utf-8"?>
<KNX xsi="http://www.w3.org/2001/XMLSchema-instance" xsd="http://www.w3.org/2001/XMLSchema" CreatedBy="ETS6" ToolVersion="6.1.5686.0">
  <ManufacturerData>
    <Manufacturer RefId="M-0083">
      <APS>
        <AP Id="M-0083_A-0138-21-F18E-O0072" ApplicationNumber="312" ApplicationVersion="33" ProgramType="ApplicationProgram" MaskVersion="MV-0012" Name="IP Interface Secure" LoadProcedureStyle="DefaultProcedure" PeiType="0" DefaultLanguage="en-US" DynamicTableManagement="false" Linkable="false" IsSecureEnabled="true" MinEtsVersion="5.0" OriginalManufacturer="M-0072" AdditionalAddressesCount="4" MaxUserEntries="5" MaxTunnelingUserEntries="4" MaxSecurityGroupKeyTableEntries="1" Hash="8egB0tSCoJMwqt1UnOQ0jg==">
          <St>
            <Code>
              <AS Id="M-0083_A-0138-21-F18E-O0072_AS-0100" Name="Default" Size="256" MemoryType="EEPROM" Address="256">
                <Data>////AHIpUBAIciBQrf9gAAD+Y2NjYwEAAAAA/zMAAAByIFByIFAAeAACAQAAAAAAAAAAAAAAd3cXFwgzAAAEAP///////////////+AAFwwAAB4AVEFQS08gS05YIFRQIElQAAAAAAAAAAAAAAAAAAAAAGQAAED/////H5AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA==</Data>
                <Mask>/wAAAP////////////////////////8AAP////////////////////////////////////////////////8AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA/////wD/////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////////AA==</Mask>
              </AS>
            </Code>
            <PTS>
              <PT Id="M-0083_A-0138-21-F18E-O0072_PT-tUINT8" Name="tUINT8">
                <TNr SizeInBit="8" Type="unsignedInt" minInclusive="0" maxInclusive="255" />
              </PT>
              <PT Id="M-0083_A-0138-21-F18E-O0072_PT-tIP432" Name="tIP432">
                <TIP AddressType="HostAddress" />
              </PT>
              <PT Id="M-0083_A-0138-21-F18E-O0072_PT-en.5FslowConnection" Name="en_slowConnection">
                <TR Base="Value" SizeInBit="8">
                  <Enumeration Text="yes" Value="0" Id="M-0083_A-0138-21-F18E-O0072_PT-en.5FslowConnection_EN-0" />
                  <Enumeration Text="no" Value="1" Id="M-0083_A-0138-21-F18E-O0072_PT-en.5FslowConnection_EN-1" />
                </TR>
              </PT>
              <PT Id="M-0083_A-0138-21-F18E-O0072_PT-en.5FfrontendProtection" Name="en_frontendProtection">
                <TR Base="Value" SizeInBit="8">
                  <Enumeration Text="settings active" Value="0" Id="M-0083_A-0138-21-F18E-O0072_PT-en.5FfrontendProtection_EN-0" />
                  <Enumeration Text="only status" Value="2" Id="M-0083_A-0138-21-F18E-O0072_PT-en.5FfrontendProtection_EN-2" />
                  <Enumeration Text="locked settings" Value="3" Id="M-0083_A-0138-21-F18E-O0072_PT-en.5FfrontendProtection_EN-3" />
                </TR>
              </PT>
              <PT Id="M-0083_A-0138-21-F18E-O0072_PT-HTTP.20Port" Name="HTTP Port">
                <TR Base="Value" SizeInBit="16">
                  <Enumeration Text="80" Value="80" Id="M-0083_A-0138-21-F18E-O0072_PT-HTTP.20Port_EN-80" />
                  <Enumeration Text="8080" Value="8080" Id="M-0083_A-0138-21-F18E-O0072_PT-HTTP.20Port_EN-8080" />
                </TR>
              </PT>
            </PTS>
            <PS>
              <P Id="M-0083_A-0138-21-F18E-O0072_P-1" Name="IP_ttl" ParameterType="M-0083_A-0138-21-F18E-O0072_PT-tUINT8" Text="IP_ttl" Access="None" Value="64" InitialValue="64">
                <M CodeSegment="M-0083_A-0138-21-F18E-O0072_AS-0100" Offset="118" BitOffset="0" />
              </P>
              <P Id="M-0083_A-0138-21-F18E-O0072_P-5" Name="IP_connRepeatDisconnect" ParameterType="M-0083_A-0138-21-F18E-O0072_PT-en.5FslowConnection" Text="Enable slow connections" Value="1">
                <M CodeSegment="M-0083_A-0138-21-F18E-O0072_AS-0100" Offset="117" BitOffset="0" />
              </P>
              <P Id="M-0083_A-0138-21-F18E-O0072_P-7" Name="IP_dns" ParameterType="M-0083_A-0138-21-F18E-O0072_PT-tIP432" Text="DNS Server" Value="0.0.0.0">
                <M CodeSegment="M-0083_A-0138-21-F18E-O0072_AS-0100" Offset="119" BitOffset="0" />
              </P>
              <P Id="M-0083_A-0138-21-F18E-O0072_P-10" Name="IP_httpPort" ParameterType="M-0083_A-0138-21-F18E-O0072_PT-HTTP.20Port" Text="HTTP port" Value="8080">
                <M CodeSegment="M-0083_A-0138-21-F18E-O0072_AS-0100" Offset="123" BitOffset="0" />
              </P>
              <P Id="M-0083_A-0138-21-F18E-O0072_P-11" Name="LK_frontendProtection" ParameterType="M-0083_A-0138-21-F18E-O0072_PT-en.5FfrontendProtection" Text="Webfrontend with activated security" Value="3">
                <M CodeSegment="M-0083_A-0138-21-F18E-O0072_AS-0100" Offset="141" BitOffset="0" />
              </P>
            </PS>
            <PRS>
              <PR Id="M-0083_A-0138-21-F18E-O0072_P-1_R-1" RefId="M-0083_A-0138-21-F18E-O0072_P-1" />
              <PR Id="M-0083_A-0138-21-F18E-O0072_P-5_R-5" RefId="M-0083_A-0138-21-F18E-O0072_P-5" />
              <PR Id="M-0083_A-0138-21-F18E-O0072_P-7_R-7" RefId="M-0083_A-0138-21-F18E-O0072_P-7" />
              <PR Id="M-0083_A-0138-21-F18E-O0072_P-10_R-10" RefId="M-0083_A-0138-21-F18E-O0072_P-10" />
              <PR Id="M-0083_A-0138-21-F18E-O0072_P-11_R-11" RefId="M-0083_A-0138-21-F18E-O0072_P-11" />
            </PRS>
            <COT CodeSegment="M-0083_A-0138-21-F18E-O0072_AS-0100" Offset="250" />
            <ADRT CodeSegment="M-0083_A-0138-21-F18E-O0072_AS-0100" Offset="22" MaxEntries="0" />
            <ASSOT CodeSegment="M-0083_A-0138-21-F18E-O0072_AS-0100" Offset="254" MaxEntries="0" />
            <Script />
            <BIs>
              <BI Id="M-0083_A-0138-21-F18E-O0072_BI-1" AddressIndex="1" AccessType="Tunneling" Text="Tunneling Channel 1" />
              <BI Id="M-0083_A-0138-21-F18E-O0072_BI-2" AddressIndex="2" AccessType="Tunneling" Text="Tunneling Channel 2" />
              <BI Id="M-0083_A-0138-21-F18E-O0072_BI-3" AddressIndex="3" AccessType="Tunneling" Text="Tunneling Channel 3" />
              <BI Id="M-0083_A-0138-21-F18E-O0072_BI-4" AddressIndex="4" AccessType="Tunneling" Text="Tunneling Channel 4" />
            </BIs>
            <Opt LegacyNoPartialDownload="true" LegacyNoOptimisticWrite="true" Reconstructable="true" DownloadInvisibleParameters="None" SupportsExtendedMemoryServices="true" SupportsExtendedPropertyServices="true" SupportsIpSystemBroadcast="true" />
          </St>
          <Dynamic>
            <ChannelIndependentBlock>
              <ParameterBlock Id="M-0083_A-0138-21-F18E-O0072_PB-3" Name="invisible" Text="invisible" Access="None">
                <ParameterRefRef RefId="M-0083_A-0138-21-F18E-O0072_P-1_R-1" InternalDescription="generated" />
              </ParameterBlock>
              <ParameterBlock Id="M-0083_A-0138-21-F18E-O0072_PB-4" Name="General" Text="General">
                <ParameterRefRef RefId="M-0083_A-0138-21-F18E-O0072_P-5_R-5" InternalDescription="generated" />
                <ParameterSeparator Id="M-0083_A-0138-21-F18E-O0072_PS-1" Text="" />
                <ParameterRefRef RefId="M-0083_A-0138-21-F18E-O0072_P-11_R-11" InternalDescription="generated" />
                <choose ParamRefId="M-0083_A-0138-21-F18E-O0072_P-11_R-11">
                  <when test="2 3">
                    <ParameterSeparator Id="M-0083_A-0138-21-F18E-O0072_PS-2" Text="The locking of the Web interface only works if &quot;Secure Commissioning&quot; is activated!" UIHint="Information" />
                  </when>
                </choose>
                <ParameterRefRef RefId="M-0083_A-0138-21-F18E-O0072_P-10_R-10" InternalDescription="generated" />
                <ParameterRefRef RefId="M-0083_A-0138-21-F18E-O0072_P-7_R-7" InternalDescription="generated" />
              </ParameterBlock>
            </ChannelIndependentBlock>
          </Dynamic>
        </AP>
      </APS>
    </Manufacturer>
  </ManufacturerData>
</KNX>